TITLE: Electrostatic Painter

REPORTS TO: Body Shop Manager

POSITION INFORMATION:

The Electrostatic Painter operates cone, disk, or nozzle-type electrostatic painting equipment to spray negatively charged paint particles onto positively charged work pieces.

DUTIES AND RESPONSIBILITIES:

*(Dealer: For each job function, check ''E'' if it is essential in your dealership or ''M'' if it is marginal.)*

E( ) M( ) Move switches and dials to start flow current and to activate conveyer and paint spraying equipment.

E( ) M( ) Turn valves and observe gauges to set pressure and to control flow of paint to each spray station.

E( ) M( ) Adjust thermostat to maintain specified temperature in paint tanks.

E( ) M( ) Inspect painted units for runs, sags, and unpainted areas.

E( ) M( ) Readjust pressure valves to control direction and pattern of spray and to correct flaws in coating.

E( ) M( ) Clean paint from ceiling and walls of booth, conveyor hooks or grid, and from disks, cones, spray heads, and hoses, using solvent and a brush.

E( ) M( ) Hand-spray parts to cover unpainted areas or apply rust preventative.

E( ) M( ) Mix paint according to specifications, using viscometer to regulate consistency according to changes in atmospheric conditions.

QUALIFICATIONS:

Ability to read and comprehend instructions and information. Working knowledge of all aspects of painting body parts and bodies of vehicles. Valid driver's license. Ability to interpret vendor catalogs. Two years of experience as a vehicle painter or apprentice. Ability to use hand and power tools and other machinery safely.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

WORKING CONDITIONS:

This is a physically demanding position. Will stand six to eight hours per shift. Will lift parts weighing up to 70 pounds. Will use hand and power tools. Will be exposed to noise, vibration, paint, dust, exhaust fumes, and other hazardous and nonhazardous materials.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

NOTE:

This is not necessarily an exhaustive list of responsibilities, skills, duties, requirements, efforts, or working conditions associated with the job. While this list is intended to be an accurate reflection of the current job, the dealership reserves the right to revise the functions and duties of the job or to require that additional or different tasks be performed when circumstances change (i.e., emergencies, changes in personnel, work load, rush jobs, or technological developments).

I have carefully read and understand the contents of this job description. I understand the responsibilities, requirements and duties expected of me. I also understand that this job description does not constitute a contract of employment nor alter my status as an at-will employee. I have the right to terminate my employment at any time and for any reason, and the dealership has a similar right.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_

Employee's Name Employee's Signature Date

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_

Supervisor's Name Supervisor's Signature Date

We are an Equal Opportunity Employer